Annual Drinking Water Quality Report
J3G Utilities, Inc/Mountain Run Community Water Supply
INTRODUCTION
This Annual Drinking Water Quality Report for calendar year 2025 is designed to inform you about your drinking water quality.  Our goal is to provide you with a safe and dependable supply of drinking water, and we want you to understand the efforts we make to protect your water supply.  The quality of your drinking water must meet state and federal requirements administered by the Virginia Department of Health (VDH). If you have questions about this report, want additional information about any aspect of your drinking water, or want to know how to participate in decisions that may affect the quality of your drinking water, please contact Chris Gilman at (804) 690-8322. 

GENERAL INFORMATION
Drinking water, including bottled drinking water, may reasonably be expected to contain at least small amounts of some contaminants.  The presence of contaminants does not necessarily indicate that water poses a health risk.  More information can be obtained by calling the Environmental Protection Agency's Safe Drinking Water Hotline (800-426-4791).
Some people may be more vulnerable to contaminants in drinking water than the general population. Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections. These people should seek advice about drinking water from their health care providers. EPA/CDC guidelines on appropriate means to lessen the risk of infection by cryptosporidium and other microbiological contaminants are available from the Safe Drinking Water Hotline (800-426-4791). 
The sources of drinking water (both tap and bottled) include wells, rivers, lakes, and springs.  As water travels over the surface of the land or through the ground, it may pick up substances, including:  microbial contaminants (bugs), inorganic chemical contaminants (salts and metals), organic chemical contaminants (natural and synthetic), and/or radioactive contaminants.  To ensure that tap water is safe to drink, the US EPA prescribes and the Virginia Department of Health enforces regulations, which limit the amount of certain contaminants in water provided by public water systems.  The Food and Drug Administration and Virginia Department of Agriculture address bottled water. 

SOURCE(S) AND TREATMENT OF YOUR DRINKING WATER
The source of your drinking water is groundwater located at Deep Well #1 located to the right of the Manor House, and Deep Well #2 located southeast of the storage tank. The drinking water is then disinfected with the addition of chlorine, and potassium permanganate is added to treat manganese & iron in raw water from Well #1. Nitrates are filtered from Well #2.
A source water assessment was completed by the Virginia Department of Health in 2018. The assessment determined that our source may be susceptible to contamination because it is located in an area that promotes migration of contaminants from land use activities of concern. More information may be obtained by contacting the water system representative listed above.  All residents will be asked to complete a cross connection questionnaire in 2025.     

DEFINITIONS 
Contaminants in your drinking water are routinely monitored according to Federal and State regulations.  The tables on the next page show the results of our monitoring.  In the tables and elsewhere in this report you will find many terms and abbreviations you might not be familiar with.  The following definitions are provided to help you better understand these terms:
Non-detects (ND) - lab analysis indicates that the contaminant is not present
Parts per million (ppm) or Milligrams per liter (mg/l) - one part per million corresponds to one minute in two years or a single penny in $10,000.
Parts per billion (ppb) or Micrograms per liter - one part per billion corresponds to one minute in 2,000 years, or a single penny in $10,000,000. 
Parts per trillion (ppt) or Nanograms per liter (nanograms/l) - one part per trillion corresponds to one minute in 2,000,000 years, or a single penny in $10,000,000,000.
Picocuries per liter (pCi/L) - picocuries per liter is a measure of the radioactivity in water.
Action Level (AL) - the concentration of a contaminant which, if exceeded, triggers treatment or other requirements which a water system must follow.
Treatment Technique (TT) - a required process intended to reduce the level of a contaminant in drinking water.
Maximum Contaminant Level, or MCL - the highest level of a contaminant that is allowed in drinking water.  MCLs are set as close to the MCLGs as feasible using the best available treatment technology.
Maximum Contaminant Level Goal, or MCLG - the level of a contaminant in drinking water below which there is no known or expected risk to health.  MCLGs allow for a margin of safety.	

WATER QUALITY RESULTS J3G Utilities samples our domestic supply for coliform bacteria monthly. There were no microbiological contaminants detected in 2025.

Exposure to Lead in drinking water can cause serious health effects in all age groups. Infants and children can have decreases in IQ and attention span. Lead exposure can lead to new learning and behavior problems or exacerbate existing learning and behavior problems. The children of women who are exposed to lead before or during pregnancy can have increased risk of these adverse health effects. Adults can have increased risks of heart disease, high blood pressure, kidney or nervous system problems.


I. Lead and Copper Contaminants

	 Contaminant   
	Units of Measurement
	Action Level
	MCLG
	Results of Samples & the  90th Percentile Value
	# of  Sites Exceeding Action level
	Action Level Exceeded (Y/N)
	Mon & Yr  
of Sample
	Typical Source of Contamination

	Lead
	ppb
	15
	0
	2.69 – 6.3 ug/L, 6.1 ug/L 
	0
	No
	7/2023
	Corrosion of household plumbing systems. 

	Copper
	ppm
	1.3
	1.3
	<0.02 – 0.274 mg/L, 0.174 
	0
	No 
	7/2023
	Corrosion of household plumbing systems.


Lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. J3G Utilities is responsible for providing high quality drinking water and removing lead pipes, but cannot control the variety of materials used in the plumbing components in your home. You share the responsibility for protecting yourself and your family from the lead in your home plumbing. You can take responsibility by identifying and removing lead materials within your home plumbing and taking steps to reduce your family’s risk. Before drinking tap water, flush your pipes for several minutes by running your tap, taking a shower, doing a load of laundry or dishes. You can also use a filter certified by an American National Standards Institute accredited certifier to reduce lead in drinking water. If you are concerned about lead in your water and wish to have your water tested, contact Chris Gilman at J3G Utilities at 804-690-8322. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available at http://www.epa.gov/safewater/lead.

II. Other Chemical and Radiological Contaminants

	 Contaminant   
	Units of Measure
	MCLG
	MCL
	Level Detected
	Range of Detection at Sampling Points
	Violation Y/N
	Month & Year  
of last Sample
	Typical Source of Contamination

	Nitrate
	ppm
	10
	10
	5.18
	1.72 – 5.18 ppm
	No
	12/2025 
	Erosion of natural deposits, or fertilizers. 

	Barium
	ppm
	2
	2
	0.085
	n/a
	No
	4/2023
	Erosion of natural deposits.  

	Total Trihalomethanes (TTHM)
	    ppb
	     n/a
	80
	3.0
	n/a
	No
	9/2025
	By-product of disinfection.

	Chlorine
	    ppm
	       4
	4
	0.34
	.22 - .55
	No
	12/2025
	Water additive to control microbes.

	 Haloacetic Acids (Haa5)
	    ppb 
	     n/a
	60
	<1
	n/a
	No
	9/2025
	By-product of disinfection.

	Flouride
	    ppm
	     n/a
	n/a
	.2
	n/a
	      No
	2023
	Erosion of natural deposits or water additive which promotes strong teeth



We constantly monitor for various contaminants in the water supply to meet all regulatory requirements. The tables list only those contaminants that had some level of detection.  Many other contaminants have been analyzed but were not present or were below the detection limits of the lab equipment.  The state allows us to monitor for some contaminants less than once per year because the concentrations of these contaminants do not change frequently.  Therefore, some of our data, though accurate, is more than one year old.
Other drinking water constituents you may be interested in: the Calcium hardness is 120 mg/L, sodium is 18.8 ppm and fluoride is < .2 ppm. People on strict sodium intake diets should avoid consuming water with sodium concentrations higher than 20 mg/L and may want to consult with their physician.  
MCLs are set at very stringent levels by the U.S. Environmental Protection Agency.  In developing the standards EPA assumes that the average adult drinks 2 liters of water each day throughout a 70-year life span.  EPA generally sets MCLs at levels that will result in no adverse health effects for some contaminants or a one-in-ten-thousand to one-in-a-million chance of having the described health effect for other contaminants.

III. Unregulated Contaminant

	Contaminant
	Units of measure
	MCLG
	MCL
	Level Detected
	Month & Year of last Sample
	Typical Source of Contamination

	Sodium
	ppm
	      N/A        
	     N/A
	18.8 
	             4/2023
	       Erosion of Natural Deposits



The service line inventory is available at TheFederalClub.com/utilities/. 
Our water system processed and distributed 7,266,550 gallons in 2025. This Drinking Water Quality Report was prepared by Chris Gilman and Vincent Lofton. 
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